{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":8,"n_cols":8,"rows_kept":8,"merged":[[0,0,0,7]],"flags":["formulas_cached_only"]}
["工作量清单报价单"]
["序号","项目","规格及参数","数量","单位","单价\n(元)","合计\n(元)","备注"]
[1,"户外小品\n(欢迎回家底座、框架)","规格：\n4500mm*1800mm（整体框架尺寸）                         1.框架主材：1.5mm镀锌方管主框架，内部增设加强筋；边框采用镀锌钢板\n2.防腐工艺：整体框架先喷砂除锈，喷涂环氧防锈底漆，表层户外氟碳静电喷塑\n3.表面颜色：按设计色号定制，色泽均匀，耐紫外线不褪色\n4.焊接工艺：满焊连接，所有焊口打磨平整，无毛刺、尖锐棱角，公共场所安全标准\n5.防水工艺：箱体拼接缝隙采用户外中性耐候硅酮密封胶满打密封，箱体底部预留Φ6mm专用排水孔，杜绝积水渗水            \n6.C25混凝土浇筑底座，底部钢架40方管钢架预埋，500*400*500mm。                            全费用综合单价，包含辅材及安装人工，平板大货车运输等等，设计+制作+安装",1,"套"]
[2,"亚克力发光字\n（欢迎回家围边、面板、加灯珠）","规格：\n850mm*850mm*4（欢迎回家尺寸）                4300mm*320mm*1（盐城城投物业LOGO尺寸） \n1050mm*560mm*1（欢迎上部帽子造型）\n340mm*310mm*1(黄色爱心尺寸)                               1.材质：户外抗UV浇注型PMMA亚克力（红色半透）\n2.板材厚度：5mm（大型景观字标准，杜绝板面变形，光线均匀扩散）\n3.光学指标：透光率38%~45%，内置光扩散粒子，无灯珠光斑、整面均匀发光\n4.耐候要求：添加紫外线稳定剂，户外2年不易发黄、褪色；\n5.加工工艺：CNC激光切割，切口抛光；面板与字壳打胶全密封防水                          \n6.围边材料：1.5mm镀锌板热切割工艺                    7.内壁处理：内壁喷哑光白色反光漆，提升光线利用率，减少暗角\n8.防水构造：箱体底部预留φ6mm排水孔；面板接缝采用中性耐候硅酮密封胶                          9.光源型号：SMD2835 防水LED模组（红色光）\n10.供电规格：DC12V 低压安全供电（户外景观强制推荐，防触电）\n11.模组排布：模组间距 80~100mm均匀排布；距离亚克力面板≥35mm，消除点状光斑\n12.防护等级：模组 IP65防水\n13. 色温/光色：主波长620–625nm 正红光\n14. 亮度：表面成品亮度450–700cd/㎡（白天可视、夜晚不刺眼，小区归家氛围适配）",1,"套"]
[3,"合计"," 含税总价\n（增值税专票税率：    %）"]
[]
[{"$nulls":5},"报价单位：（盖章）"]
[{"$nulls":5},"日期："]